# ID 50499

Spindle speed is 0.
Description | With turning functions revolution feedrate G95 and thread cutting G33, he path feedrate is derived from the programmed spindle speed. For this reason, the spindle speed programmed via the S word must not be 0 for the active turning functions mentioned above.

For further information see [PROG// Section: Turning functions].

Response | Class | 6 | Movement stop.
Solution | Class | 6 | Program spindle speed > 0!
Error type | 1, Error message from NC program.