# ID 110075

Parameters for position controller and interpolator incomplete.
Description | The machine data record was not completely initialised. This can only happen if this data record is transferred in binary form to the CNC.
Response | Class | 3 |
Solution | Class | 7 |
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Incorrect value [-]
Incorrect bitmask
Error type | 2, Error message on data transfer of parameter lists to controller.