# Settings for vector dynamic limits (vector.*)

The maximum permissible velocity, acceleration and deceleration on the path are dependent on the dynamic values in the axis-specific parameter list and the programmed contour. The following parameters initialise path velocity and acceleration/deceleration default limits. Activation/deactivation and change of limits are executed by NC command (see also [PROG//Command #VECTOR LIMIT..]).

## Additional information

- Vector acceleration limit (P-CHAN-00002)
- Path deceleration limit (P-CHAN-00208)
- Radial acceleration limit (P-CHAN-00361)
- Unit for path acceleration/deceleration and jerk (P-CHAN-00351)
- Path velocity limit (P-CHAN-00090)
- Dynamic limit in the circle (P-CHAN-00350)