# Measure slot in X axis

After positioning within the slot, the touch probe measures both in the positive and negative X directions. The touch probe must be positioned at measuring depth as centrally as possible in the slot either manually or in automatic mode.

Measure slot in X axis

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables