# Enable 2-path programming (P-CHAN-00261)

P-CHAN-00261 | Enable 2-path programming
Description | This parameter enables the NC syntax for 2-path programming. It permits the programming of two synchronous motions (paths) for 2 axis groups in the same NC block. The motions are separated in the NC block by a colon ':‘. <global> <separator> <path1> <separator> <path2>

Nxx G01 G90 F100 : X100 Y100 Z0 : U100 V100 W0

Parameter | multi_path_configuration
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | When 2-path programming is active, the colon ‘:’ signifies a separator in the syntax. Jump marks to block numbers Nxx: (also called expression labels) is not possible, but only jumps on string labels are allowed.