# ID 110505

Changing parameters of axis-specific current values transformation requires restart of the control.
Description | An attempt was made to change the value of P-AXIS-00382 with an update of the axis parameter list. This is not possible; a change of P-AXIS-00382 requires a controller restart.
Response | Class | 1 | Warning output, the value of P-AXIS-00382 will not be changed.
Solution | Class | 1 | Change parameter and restart control.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis
%2: | Current value [-]
Changed value of P-AXIS-00382
%3: | Corrected value [-]
Old value of P-AXIS-00382
Error type | 2, Error message by data transfer from parameter list into control device.