# ID 50727

Axis number in drive command not found.
Description | The axis number specified in a #DRIVEcommand was not found.
Response | Class | 6 | Program execution stop.
Solution | Class | 6 | Correct NC program. The axis number programmed has to be known in the NC channel. When the function 'Insertion of NC program[FCT-C15]’ is used, the channel parameter P-CHAN-00282 can be used to specify whether the axis numbers of the axis in the clone channel or the axis numbers of the axis in the master channel are to be used.
Parameter | %1: | Logical axis number [-]
Axis number of axis not found.
%2: | Current value [-]
Value of the channel parameter P-CHAN-00282.
Error type | 1, Error message from NC program.