# Overview of channel and axis parameters

ID | Description
--- | ---
P-CHAN-00406 | Enable realtime cycle functionality
P-CHAN-00407 | Memory for real-time cycles
P-CHAN-00424 | Memory size for V.CH. variables
P-CHAN-00425 | Max. execution time of realtime cycles per CNC cycle
P-CHAN-00426 | Number of elementary instructions for time check
P-CHAN-00427 | Max. number of elementary instructions per CNC cycle
P-CHAN-00480 | Max. number of actions within a real-time cycle

ID | Description
--- | ---
P-AXIS-00457 | Enable PLCopen interface of a channel axis