# Parameters

Cycle parameters | Description
@P6 | Measurement path in the Z axis (incremental) Positive value, the touch probe moves in positive Z direction Negative value, the touch probe moves in negative Z direction
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P11 (optional) | Shift the measuring point along the Z axis