# ID 294060

The motor temperature indicated greater than 155 degrees centigrade.
Description | The motor temperature of the displayed axis is more than 155°C. (Signalling is done by PTC element in the motor winding)
Response | Class | 7 | Path-maintaining braking. All active commands inhibited.
Solution | Class | 6 | Reduce mechanical load. Rectify any faults.
Error type | 11, Error message from position controller.