# ID 110125

Maximum velocity for manual mode may not be 0.
Description | The maximum velocity P-AXIS-00213 with active manual mode is set to zero. The maximum velocity is set to default value.
Response | Class | 1 | None.
Solution | Class | 1 | Set maximum velocity for manual mode P-AXIS-00213 to greater than 0.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [1µm/s or 0.001°/s]
Current maximum velocity P-AXIS-00213.
%3: | Corrected value [1µm/s or 0.001°/s]
Corrected maximum velocity P-AXIS-00213.
Error type | 2, Error message on data transfer of parameter lists to controller.