# Outer diameter with four points

The touch probe is positioned above the workpiece. Then, measurements take place in the positive and negative directions of the X and Y axes. This requires repeated pre-positioning in each case. The touch probe must be positioned as centrally as possible above the spigot either manually or in automatic mode.

Outer diameter with four points

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables