# ID 20226

'ENDSWITCH' must be programmed exclusively in NC-block.
Description | In the same NC block, a control block instruction was programmed with further NC commands. After a $ENDSWITCH no further NC commands may be programmed. Example: Wrong: N10 G00 X0 Y0 Z0 N20 P1=5

N50 $SWITCH P1

:

N62 $DEFAULT

:

N65 $ENDSWITCH G01 X100 F10000

:

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 P1=5

N50 $SWITCH P1

:

N62 $DEFAULT

:

N65 $ENDSWITCH

N66 G01 X100 F10000

:

N1000 M30

For further information see [PROG// Section: Switch branching]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Move the not permissible NC commands after $ENDSWITCH to other NC blocks or delete them.
Error type | Abort NC program processing.