# ID 294060

The motor temperature indicates greater than 155 degrees centigrade.
Description | The motor temperature of the displayed axis is more than 155°C (signal output by PTC element in the motor winding.)
Response | Class | 7 | Contour-accurate stop. All active commands inhibited.
Solution | Class | 6 | Reduce mechanical load. Rectify any faults.
Error type | 11, Error message from position controller.