# ID 294027

General drive error, see parameter 4.
Description | The DSE-drive reports a general error.
Response | Class | 7 | Stop the axis. All active commands inhibited.
Solution | Class | 6 | Contact the service personnel. Eliminate error. Reset the fault on the DSE-module.
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis.
%2: |
DSE drive address.
%3: |
DSE error id.
%4: | Current value [-]
Error Number.
Error type | 11, Error message from position controller.