# ID 70288

Configured data type is not supported.
Description | The data type of a configured drive function is not supported.
Response | Class | 1 | Program execution stop.
Solution | Class | 1 | Change configuration, use a communication type that is supported for this drive type.
Parameter | %1: | Current value [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Current value [-]
Name of drive function
%3: | Error value [-]
Data type not supported.
Error type | 11, Error message from position controller.