# ID 110581

Change of P-AXIS-00511 requires a restart.
Description | The value P-AXIS-00511 should be changed by updating a parameter list, this is only permitted if the bit "ALLOW_RESOLUTION_CHANGE" is set in P-AXIS-00015.
Response | Class | 0 | Error message output, new value is not accepted.
Solution | Class | 0 | In parameter P-AXIS-00015 set the bit "ALLOW_RESOLUTION_CHANGE" or change P-AXIS-00511 by controller restart.
Parameter | %1: |
Axis number
%2: |
Set value of P-AXIS-00511.
%3: |
Corrected (old) value of P-AXIS-00511.
Error type | -