# ID 110419

Changing of parameter encoder_range requires restart of the control.
Description | The parameter P-AXIS-00296 for the range of the position sensor cannot be changed while the CNC kernel is running. The modified value is not adopted; the previous value remains valid.
Response | Class | 0 | None.
Solution | Class | 0 | Change the sign P-AXIS-00296 in configuration mode or when the CNC is inactive.
Parameter | %1: |
Logical axis number P-AXIS-00016 of axis affected.
%2: |
Current value of P-AXIS-00296.
%3: |
Corrected value of P-AXIS-00296.
Error type | -