# ID 110560

Position window for rapid movement can not be used with spindles.
Description | For a spindle (see P-AXIS-00018), a value > 0 has been parameterized for axis parameter P-AXIS-00472. The parameter P-AXIS-00472 cannot be used with spindles, because spindles cannot be moved with rapid movements.
Response | Class | 1 | Warning output, P-AXIS-00472 is set to zero (nil).
Solution | Class | 1 | P-AXIS-00472 has a value <= 0.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Parameterized value of P-AXIS-00018.
%3: | Error value [-]
Parameterized value of P-AXIS-00472.
%4: | Corrected value [-]
Corrected value of P-AXIS-00472.
Error type | 2, Error message by data transfer from parameter list into control device.