# ID 110393

acceleration for homing greater than maximum permissible value.
Description | The acceleration for the homing P-AXIS-00285 with jerk limited slope was specified to be greater than the maximum permissible acceleration P-AXIS-00008.
Response | Class | 1 | Limitation of acceleration with maximum value
Solution | Class | 1 | Setting of acceleration for homing smaller than maximum value.
Parameter | %1: | Logical axis number [-]
Logical axis number of concerned axis P-AXIS-00016.
%2: | Current value [1mm/s^2 or 1°/s^2]
Current acceleration P-AXIS-00285.
%3: | Upper limit value [1mm/s^2 or 1°/s^2]
Maximum permissible acceleration P-AXIS-00008.
%4: | Corrected value [1mm/s^2 or 1°/s^2]
Corrected acceleration P-AXIS-00285.
Error type | 2, Error message by data transfer from parameter list into control device.