# Conditional filter activation (P-STUP-00190)

P-STUP-00190 | Conditional filter activation
Description | The individual error codes can be listed as numbers or texts, whereby the entire row must comply with the following syntax: ( number | text ) {, ( number | text ) } where: number:= CNC error number text := " error-specific text "
Parameter | error_filter[i].conditional_param where i = 0 ... 3 (maximum number of filters, application-specific)
Data type | STRING
Data range | Maximum of 96 characters
Dimension | ----
Default value | *
Remarks | Parameterisation example: error_filter[0].conditional_param "D012:", 123, 1001 Individual error texts are only checked when the SERCOS drive error S95 is read out. Error numbers are only checked in case of SERCOS drive errors (S21 and S22) and in case of ProfiDrive drive errors (parameter 945).

* Note: The default value of variables is a blank string.