# ID 110418

Value for parameter encoder_range is outside permissible range.
Description | Parameter P-AXIS-00296 is out of the permissible range.
Response | Class | 1 | Warning output, correct the value of P-AXIS-00296. If P-AXIS-00296 was configured below the minimum value, P-AXIS-00296 is set to the minimum value, otherwise, if the maximum value was exceeded, P-AXIS-00296 is limited to the maximum value.
Solution | Class | 1 | Set a valid value for P-AXIS-00295 in the axis parameter list.
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis (see P-AXIS-00016).
%2: | Current value [-]
Index of the invalid entry in the lr_hw[] array. A value of 0 means lr_hw[0].encoder_range is incorrect.
%3: | Lower limit value [-]
%4: | Upper limit value [-]
%5: | Corrected value [-]
Error type | 2, Error message on data transfer of parameter lists to controller.