# ID 60273

Stability reserve of designed filter not sufficient.
Description | It is not possible to design a stable filter for all filter parameters, e.g. due to the limited calculation accuracy. Possible solutions are:

- Reduce order P-AXIS-00140 of the filter
- Reduce the reciprocal bandwidth P-AXIS-00080 of band-pass or band-stop filters
- Choose a different filter prototype P-AXIS-00153
- Increase the ratio of cut-off frequency to sample rate

Response | Class | 3 | Filter is deactivated
Solution | Class | 7 | Change filter parameters
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis
%2: |
Number of concerned filter
%3: |
Filter typer P-AXIS-00204
%4: |
Filter order P-AXIS-00140
%5: |
Filter cut-off frequency P-AXIS-00067 or time constant P-AXIS-00357 of PT1 filter/PT2 filter
Error type | -