# ID 70384

The scaled limit value is smaller than the minimum value of the configured data type.
Description | The scaled (see P-AXIS-00401) value of parameter P-AXIS-00408 is smaller than the minimum value of the data type set with parameter P-AXIS-00399.
Response | Class | 1 | Warning output, P-AXIS-00408 is automatically limited to the minimum value according to P-AXIS-00399.
Solution | Class | 1 | P-AXIS-00408 value must be adjusted.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Value of P-AXIS-00396 for identification of drive function.
%3: | Error value [-]
Parameterized value of P-AXIS-00408.
%4: | Current value [-]
Scaling factor (see P-AXIS-00401).
%5: | Limit value [-]
Minimum possible value for P-AXIS-00408 taking into account P-AXIS-00399 and P-AXIS-00401, simultaneously corrected value.
Error type | 11, Error message from position controller.