# ID 70333

Axis was released with active distance control.
Description | The axis was released (#PUT AX) but distance control is still active (see [FCT-M3]). Before axis release, distance control must be switched off.
Response | Class | 7 | Immediate axis stop. Distance control is turned off.
Solution | Class | 6 | Deactivate distance control before axis release
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
%2: | Block number [-]
Block number in the CNC program where the error occurred
%3: | Error value [-]
Current correction offset of distance control
%4: | Current value [-]
Current state of distance control
Error type | 11, Error message from position controller.