# Axis assignment of data in the clamp position offset group (pzv_grp[i].achse[j.*])

This structure element assigns clamp position offsets to path axes. The axis index corresponds to the channel-internal axis index.

Structure name | Index
achse[j] | j = 0 ... 31 (maximum number of axes per channel: 32, application-specific)

## Additional information

- Axis-specific clamp position offset (P-CLMP-00001)