# ID 110320

Unknown entry in configuration of output telegram.
Description | At CNC kernel start-up, entries in the axis parameter lists are assigned between the data transferred cyclically to or from the drive and the internal working data of the CNC. An unknown value was detected in one of these entries. In the following example, either value 99999 in entry antr.terminal.out[1].signal_nr or value XXXXXX in entry antr.terminal.out[1].nc_ref is invalid.

Example:

antr.terminal.out[1].signal_nr 99999
antr.terminal.out[1].signal_len 2
antr.terminal.out[1].nc_ref XXXXXX

Response | Class | 3 | Error message output, invalid entry is ignored.
Solution | Class | 6 | Correct invalid entry in the parameter list.
Parameter | %1: | Current value [-]
P-AXIS-00020
%2: | Current value [-]
P-AXIS-00016
%3: | Logical axis number [-]
Index of the invalid entry, in the above example 1.
%4: | Current value [-]
Signal number of the incorrect entry, in the above example 99999.
%5: | Current value [-]
Signal name of the incorrect entry, in the above example XXXXXX.
Error type | -