# ID 110588

The specified, relevant measuring edge is invalid.
Description | In parameter P-AXIS-00518 "kenngr.measure.edge", the relevant measuring edge for a measurement run (e.g. G100) is defined. However, the setting found is invalid. Correct values are POS (positive edge) or NEG (negative edge).
Response | Class | 1 | Warning and correction of parameter P-AXIS-00517
Solution | Class | 1 | Correct the parameter P-AXIS-00518 for the relevant measuring edge.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Drive type [-]
Drive type P-AXIS-00020 of the axis
%3: | Current value [-]
Selected measuring signal source P-AXIS-00516
%4: | Error value [-]
Incorrect value for relevant measuring edge P-AXIS-00518
%5: | Corrected value [-]
Corrected value for relevant measuring edge P-AXIS-00518
Error type | 2, Error message by data transfer from parameter list into control device.