# ID 70357

Invalid probing channel programmed.
Description | With a NC command “MC_TouchProbeChannel” (see also [PROG] a channel number was specified but lies outside of the valid range.
Response | Class | 7 | Error message output, abort NC program.
Solution | Class | 6 | Use correct channel number.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
%3: | Lower limit value [-]
%4: | Upper limit value [-]
%5: | Error value [-]
Error type | 11, Error message from position controller.