# Weighting factor for ramp time (P-CHAN-00194)

P-CHAN-00194 | Weighting factor for ramp time (path-dependent dynamic weighting)
Description | This parameter defines the weighting factor for ramp time under index i.
Parameter | dynamic_weighting[i].ramp_time_fact
Data type | UNS32
Data range | 10 < ramp_time_fact < MAX(UNS32)
Dimension | 0.1%
Default value | 0
Remarks | Either the rapid traverse ramp time and/or G01 ramp time is weighted depending on P-CHAN-00190.