# ID 70324

Encoder overflow offset bigger than encoder range.
Description | The shift of the encoder overflow (P-AXIS-00354) is greater than the distance moved within one encoder revolution (P-AXIS-00355).
Response | Class | 5 | Axis stop
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Error value [0.1 µm or 0.0001°]
Parameterised value of P-AXIS-00354.
%3: | Limit value [0.1 µm or 0.0001°]
Limit value for P-AXIS-00354.
%4: | Corrected value [0.1 µm or 0.0001°]
Corrected value of P-AXIS-00354
Error type | 6, Error message by data transfer to control device.