# ID 21919

Inserting the programmed chamfer not possible.
Description | The programmed chamfer cannot be inserted. Causes:

- the programmed chamfer is too long or
- At least one of the adjacent motion blocks between which the chamfer is programmed is too short.

Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | Check and modify the NC program:

- Reduce length of chamfer
- Extend the motion blocks adjacent to the chamfer

Parameter | %1: | Error value [0.1 µm or 0.0001°]
Programmed length of chamfer
%2: | Upper limit value [0.1 µm or 0.0001°]
Maximum possible chamfer length
Error type | 1, Error message from NC program.