# ID 50010

Motion path of the measurement block is too small.
Description | To use edge bending function G108 , the probe hardware has to be initialized before entered the first movement block and after programmed MNE_SNS M code. The travelling distance is too small for initialisation of the probe hardware. For detailed information on measurement function G108, see [PROG// Section: Edge bending].
Response | Class | 6 | Movement stop.
Solution | Class | 6 | Check path distance in measurement block; short blocks may occur due to contour-changing functions such as TRC, polynomial smoothing etc.
Error type | 1, Error message from NC program.