# ID 110062

Modification of the logical axis number requires a restart.
Description | The parameter @@P-AXIS-00016 for unique identification of an axis in system cannot be changed while CNC kernel is running. The new logical axis number is not transferred, the previous active logical axis number remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Only change logical axis number P-AXIS-00016 in configuration mode or if CNC does not run respectively.
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016
%2: | Current value [-]
Current value of P-AXIS-00016.
%3: | Corrected value [-]
Corrected value of P-AXIS-00016.
Error type | 2, Error message by data transfer from parameter list into control device.