# ID 50045

Setting the manual mode parameters not possible.
Description | It is not possible to parameterise the axis for manual mode. For additional information on manual operation mode, see [PROG// Section: Manual mode], [HL// Section: Manual mode].
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Check if the axis or axes is/are available in the NC channel. Check the parameterisation of the manual mode axes in the NC program or PLC program.
Error type | 1, Error message from NC program.