# Average value filter for current master velocity (P-AXIS-00300)

P-AXIS-00300 | Average value filter for current master velocity for camming / gearing
Description | This parameter activates the arithmetic average value filter for the mast actual velocity. 0 – inactive 1 – active This parameter is used for gearing at the current master velocity.
Parameter | cam_gear.mv_type
Data type | UNS16
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | ----
Remarks |