# ID 20685

When specifying the dwell time, additional axes have been programmed.
Description | When programming the dwell time via G04, more than the first main axis in NC block is used for defining the dwell time. Example: Wrong: N10 G00 X0 Y0 Z0 N20 G04 X2 Y3

:

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 G04 X2

:

N1000 M30

Alternatively, dwell time is programmable using the command #TIME.

Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | Check and modify NC program. With G04, only the first main axis may be used for the assignment of the dwell time. Remove redundant axes programmings.
Parameter | %1: | Logical axis number [-]
Number of the redundant axis
Error type | 1, Error message from NC program.