# ID 20851

Double programming of spindle position.
Description | The position of a spindle has been programmed several times, this is not allowed with the spindle-specific (POS) or DIN syntax (S.POS).
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and remove the multiple programmed spindle position.
Parameter | %1: | Current value [0.1 µm or 0.0001°]
Error type | 1, Error message from NC program.