# ID 20977

Double programming of deceleration adjustment.
Description | The deceleration adjustment was programmed several times in the same NC block. It is not permissible to program commands G09, G900 or G901 combined in one NC block.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Modify the NC program.
Parameter | %1: | Error value [-]
Error type | 1, Error message from NC program.