# ID 70182

Invalid logical axis number for plane compensation.
Description | The logical axis number of the first or second master axis for plane compensation is invalid, since its value is zero (nil) or does not exist. The axes, whose actual positions influence the correction value, are named master axes. The function is switched off for the specified axis (see P-AXIS-00174).

See also [FCT-C5// Section: Plane compensation]

Response | Class | 7 | Closed-loop controlled axis stop. The plane compensation is turned off for affected axis.
Solution | Class | 7 | Correct logical axis number of master axis see P-COMP-00014 and P-COMP-00015
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Logical axis number [-]
Logical axis number of first master axis see P-COMP-00014
%3: | Logical axis number [-]
Logical axis number of second master axis see P-COMP-00015
Error type | 2, Error message by data transfer from parameter list into control device.