# ID 50262

Virtual and other axes are take part mixed at measurement.
Description | When using measurement function G100, virtual axes and axes of another drive type (P-AXIS-00020) are mixed in measurement axes group. This is not permitted. For more information on the G100 measuring function see [PROG// Section: Measuring functions]

[FCT-C4].

Response | Class | 4 | Movement stop.
Solution | Class | 6 | Use either all axes of measurement group with drive type virtual or all measurement run with other drive type (P-AXIS-00020).
Parameter | %1: | Current value [-]
Number of measurement axes in measurement group.
%2: | Current value [-]
Programmed axes of measurement axis group.
Error type | 1, Error message from NC program.