# MCV_DeactivateAxis

The FB deactivates or parks an axis. In this state it is no longer possible to move the axis and no further error messages are displayed.

The axis is activated by default

Blockdiagramm

Parameters of the FB

VAR_IN_OUT
Variable name | Data type | Description
axis | AXIS_REF | Axis reference

VAR_INPUT
Variable name | Data type | Description
enable | BOOL | Is TRUE when the axis is deactivated.

VAR_OUTPUT
Variable name | Data type | Description
IsDeactivated | BOOL | Is TRUE when the axis is deactivated.
Error | BOOL | Indicates TRUE if an error occurs in the FB.
ErrorID | WORD | Error code.