# ID 13110

Machining depth not defined.
Description | The machining depth must be defined either as absolute or as relative. This message is generated if neither of the two data input parameters for the machining depth is assigned for absolute or relative entries.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Define whether the machining depth is to be defined as absolute or relative and program the input parameters accordingly.
Error type | Error message from NC cycle