# Resettable path distance (P-AXIS-00072)

P-AXIS-00072 | Resettable path distance
Description | Maximum permissible path distance between master and slave gantry axes. Error that can be remedied by NC reset.
Parameter | kenngr.gantry_max_diff_resetable
Data type | UNS32
Data range | 0 < gantry_max_diff_resetable < MAX(UNS32)
Axis types | T, R
Dimension | T: 0.1 µm | R,S: 0.0001°
Default value | 0
Drive types | ----
Remarks |