# Offset of temperature compensation (P-AXIS-00274)

P-AXIS-00274 | Parameterisation of temperature compensation (Geometrical pitch)
Description | The compensation values are approximated by a straight line. This straight line is defined by a basic position, an offset at this position and a geometrical pitch. Depending on the temperature these parameters can be adjusted e.g. by the PLC.
Parameter | lr_param.temp_comp_coefficient
Data type | REAL64
Data range | -10000 ≤ temp_comp_coefficient ≤ 10000
Axis types | T, R, S
Dimension | T: µm/m | R,S: ----
Default value | 0
Drive types | ----
Remarks |