# ID 60212

Velocity for the movement is 0.
Description | The programmed velocity for the movement is less than the minimal permissible velocity.
Response | Class | 6 | Program is aborted
Solution | Class | 6 | Modify the NC program.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [1µm/s or 0.001°/s]
Programmed velocity
%3: | Limit value [1µm/s or 0.001°/s]
Permissible minimum velocity
%4: | Current value [-]
Error type | 1, Error message from NC program.