# Filter - bandwidth (P-AXIS-00080)

P-AXIS-00080 | Bandwidth of axis specific command value filter
Description | Definition of reciprocal of bandwidth for band-pass and band-stop filter types. The figure below illustrates the parameter behaviour.
Parameter | filter[i].guete
Data type | REAL64
Data range | 1 ≤ guete ≤ 10
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 1.0
Drive types | ----
Remarks |