# ID 120679

Program end while SYNC IN is active.
Description | With Synchronising an axis in coordinated motion (SYNC IN / OUT) the area must be ended by SYNC OUT. In this case, the program was simply ended; this is not permissible.
Response | Class | 2 | 1, Error message from NC program.
Solution | Class | 3 | Check and modify the NC program. End synchronisation by SYNC_OUT.
Error type | 1, Error message from NC program.