# ID 110619

Given setting 'Drive disable on bus error' is not supported for this drive type.
Description | The parameter @@P-AXIS-00542 is used for CANopen drives to set the behaviour in case of a bus error. However, the parameter was set for another drive type to ("ON" or “OFF”) although the configured drive type does not support this setting.
Response | Class | 1 | Warning output, correction of P-AXIS-00542.
Solution | Class | 1 | P-AXIS-00542 must be set to "DEFAULT".
Parameter | %1: | Current value [-]
Parameter number P-AXIS-00542
%2: | Logical axis number [-]
Axis number (P-AXIS-00016)
%3: | Drive type [-]
Drive type (P-AXIS-00020)
%4: | Error value [-]
Parameterized value of P-AXIS-00542.
%5: | Corrected value [-]
Corrected value of P-AXIS-00542.
Error type | 2, Error message by data transfer from parameter list into control device.