# ID 70211

Master axis for cross compensation not present.
Description | The specified master axis for cross compensation does not exist. See also [FCT-C5// Section: Cross compensation]
Response | Class | 7 | Controlled stop of axis affected
Solution | Class | 7 | Specify a valid logical axis number, see P-COMP-00005
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis, see P-AXIS-00016
%2: | Logical axis number [-]
Specified logical axis number of the master axis which does not exist. (seeP-COMP-00005)
%3: | Drive type [-]
Drive type of axis affected, see P-AXIS-00020
%4: | Block number [-]
Block number of the NC program where the error occurred
Error type | 2, Error message by data transfer from parameter list into control device.